|  |  |
| --- | --- |
| Project:  | Wall Mounted Toilet |
| Location:  |    |
| Firm:  | J F Taylor Enterprises Ltd. |
| Date:  | 2022/12/15 |

|  |  |
| --- | --- |
| **WC-7** | TOILET - WALL-HUNG |
|  |

|  |
| --- |
| American Standard 2882107.020 7381740-200.0020A Toilet - GLENWALL®, Tank type Toilet, Wall-hung with wall outlet, High Efficiency HET 4.8 LPF (1.28 GPF), White finish Vitreous china, EverClean® antimicrobial surface, Elongated bowl.Centoco 820STSFE-001 Seat - FAST-N-LOCK, For elongated bowl, Open front, Polypropylene, Toilet seat, With seat cover, and Plastic commercial check hinges, White finish, FAST-N-LOCK mounting system takes the guess work out when tightening the hardware. The specially designed fasteners in click" when the appropriate torque is reached. The bolt and nut material shall be stainless steelJay R. Smith 0210L Carrier  |

 |

|  |  |
| --- | --- |
| **WC-8** | TOILET - WALL-HUNG |
|  |

|  |
| --- |
| American Standard 3351101.020 Toilet - AFWALL® MILLENNIUM™ FloWise®, Toilet, Wall-hung with wall outlet, Toilet operates in the range of 4.2 to 6.0 LPF (1.1 - 1.6 GPF), White finish Vitreous china, EverClean® antimicrobial surface, Elongated bowl.Centoco 1500STSCCFE-001 Seat - FAST-N-LOCK, For elongated bowl, Open front, Polypropylene, Toilet seat, Less seat cover, and Plastic commercial check hinges, White finish, FAST-N-LOCK mounting system takes the guess work out when tightening the hardware. The specially designed fasteners in click" when the appropriate torque is reached. The bolt and nut material shall be stainless steelSloan SL-ROYAL 111-1.28 Flush Valve - ROYAL® Manual Exposed Water closet flushometer, constructed from Semi-red brass, Polished chrome finish, High Efficiency 4.8 LPF (1.28 GPF).Jay R. Smith 0210L Carrier  |

 |

|  |  |
| --- | --- |
| **WC-9** | TOILET - WALL-HUNG |
|  |

|  |
| --- |
| American Standard 3351101.020 Toilet - AFWALL® MILLENNIUM™ FloWise®, Toilet, Wall-hung with wall outlet, Toilet operates in the range of 4.2 to 6.0 LPF (1.1 - 1.6 GPF), White finish Vitreous china, EverClean® antimicrobial surface, Elongated bowl.Centoco 1500STSCCFE-001 Seat - FAST-N-LOCK, For elongated bowl, Open front, Polypropylene, Toilet seat, Less seat cover, and Plastic commercial check hinges, White finish, FAST-N-LOCK mounting system takes the guess work out when tightening the hardware. The specially designed fasteners in click" when the appropriate torque is reached. The bolt and nut material shall be stainless steelSloan SL-ROYAL 111-1.28-ESS Flush Valve - ROYAL® Automatic no-touch Exposed Water closet flushometer, Hardwired, constructed from Semi-red brass, Polished chrome finish, High Efficiency 4.8 LPF (1.28 GPF).Sloan SL-EL-154 Faucet and Flush Valve Power Kit - For flush valveJay R. Smith 0210L Carrier  |

 |

|  |  |
| --- | --- |
| **WC-10** | TOILET - WALL-HUNG |
|  |

|  |
| --- |
| American Standard 3353101.020 Toilet - AFWALL® MILLENNIUM™ FloWise®, Toilet, Wall-hung with wall outlet, Toilet operates in the range of 4.2 to 6.0 LPF (1.1 - 1.6 GPF), White finish Vitreous china, EverClean® antimicrobial surface, Elongated bowl.Centoco 1500STSCCFE-001 Seat - FAST-N-LOCK, For elongated bowl, Open front, Polypropylene, Toilet seat, Less seat cover, and Plastic commercial check hinges, White finish, FAST-N-LOCK mounting system takes the guess work out when tightening the hardware. The specially designed fasteners in click" when the appropriate torque is reached. The bolt and nut material shall be stainless steelSloan SL-ROYAL 140-1.28-WB-ESS Flush Valve - ROYAL® Automatic no-touch Concealed Water closet flushometer, Hardwired, constructed from Semi-red brass, Rough brass finish, High Efficiency 4.8 LPF (1.28 GPF).Sloan SL-EL-154 Faucet and Flush Valve Power Kit - For flush valveJay R. Smith 0210L Carrier  |

 |